|  |  |  |  |
| --- | --- | --- | --- |
| **Assessor** | Safety Security and Training for TNS | **Date** |  |
| **Description** | Working with Asbestos | **Review period** | 12 months |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Task** | **Hazard** | **Risk** | **Persons at risk** | **Risk**  **Level**  **(L x C)** | **Control measures** | **Residual Risk Level**  **(L x C)** | **Action by** | **Date completed** |
| Removal of thermal lagging / decoration of structural walls / partitions which may be cut or broken, or are allowed to deteriorate and break down. | Inhalation of asbestos fibres where the asbestos-containing materials (ACMs) are disturbed. | Death, lung disease | Staff, visitors,  volunteers,  consultants, contractors | 5 x 5 = 25 | * Ensure that an Asbestos Survey has been carried out by a specialist company, and that appropriate control measures to prevent asbestos fibres from being released have been taken. * Ensure that no building maintenance work or redecoration is carried out without reference to the Asbestos Register and survey report. * Ensure that all staff are aware of the location of ACMs and awareness training is given to all staff who are likely to come into contact with ACMs. | 2 x 5 =10 | Church Elders | At the start of every new contract |
| Drilling holes, minor repairs, any intrusion into the fabric of the building | Inhalation of asbestos fibres where the asbestos-containing materials (ACMs) are disturbed. | Death, lung disease | Staff, visitors,  volunteers,  consultants, contractors | 5 x 5 = 25 | * ACMs to be identified by signage. * Any person undertaking maintenance work to have completed Asbestos Awareness Training. | 3 x 5 =15 | Church Elders | Immediately |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name and position |  | Signature |  | Date completed |  |